Generator Mechanic (Levels 1 & 2) (Class Size: 25 Trainees)
TRADE-WISE BASELINE VERIFICATION PROFORMA
Technical Evaluation Criteria
[bookmark: _Hlk234805783]Name of Institute: _________________________________________
Procurement Entry Code: __________________________________
Address: __________________________________________________________________________________________________________________________________________________________________________________________________________Contact Number and Email: ________________________________________________________
PART-I
Mandatory Requirements (Pass / Fail)
Failure to comply with any one of the following requirements shall render the institute Technically Non-Responsive.
	S#
	Mandatory Requirement
	Verification
	Status (Pass / Fail)

	1
	Relevant Lead Trainer available during physical verification with documentary proof of employment/engagement.
	Physical
	

	2
	Dedicated Generator Mechanic Workshop, Engine Overhauling Area, Electrical Testing Laboratory and Theory Classroom available.
	Physical
	

	3
	Minimum 80% of essential workshop equipment available and fully functional.
	Physical
	

	4
	Minimum 80% of essential tools, testing instruments and diagnostic equipment available and functional.
	Physical
	

	5
	Three-phase electricity supply, adequate ventilation, fire extinguishers, first aid facilities, emergency exits and PPE available.
	Physical
	


PART-II
Technical Evaluation (75 Marks)
A. Tutor Qualification & Experience (20 Marks)
	Requirement
	Marks
	Obtained

	B.E./B.Sc. Electrical Engineering, Mechanical Engineering, Mechatronics Engineering or DAE (Electrical/Mechanical) or equivalent relevant qualification
	6
	

	Bachelor's/Master's Degree in relevant discipline (Preferred)
	2
	

	Minimum 3 years teaching/training experience in Generator Mechanics, Diesel Engines or Industrial Equipment Maintenance
	3
	

	Minimum 5 years industrial experience in installation, maintenance, overhaul and troubleshooting of diesel generator sets
	4
	

	OEM / Professional Certification (Cummins, Perkins, Caterpillar, FG Wilson, Kirloskar, Honda, Yamaha or equivalent)
	2
	

	Demonstration of practical generator maintenance, troubleshooting and testing during verification
	3
	

	Total
	20
	


B. Building Infrastructure (10 Marks)
	Facility
	Marks
	Obtained

	Theory Classroom (700–800 sq.ft.)
	1
	

	Generator Mechanic Workshop (Minimum 1,500 sq.ft.)
	3
	

	Engine Overhauling & Assembly Area
	2
	

	Electrical Testing & Control Panel Laboratory
	1
	

	Battery Charging & Electrical Systems Area
	1
	

	Tool Room & Spare Parts Store
	1
	

	Workshop Ventilation, Exhaust, Lighting and Safety Arrangements
	1
	

	Total
	10
	


C. Major Equipment (20 Marks)
	Equipment
	Minimum Quantity
	Marks
	Obtained

	Diesel Generator Sets (5–50 kVA or equivalent, different models)
	3
	3
	

	Portable Petrol Generator Sets
	2
	1
	

	Diesel Engine Training Units / Cut Sections
	2
	2
	

	Generator Alternator Training Units
	2
	2
	

	Automatic Voltage Regulator (AVR) Demonstration Units
	2
	1
	

	Generator Control Panel Training Unit (AMF/Manual)
	1
	2
	

	Generator Load Bank / Load Testing Arrangement
	1
	2
	

	Battery Charging Unit
	1
	1
	

	Air Compressor
	1
	1
	

	Engine Crane / Chain Block
	1
	1
	

	Heavy-duty Work Benches with Bench Vices
	10 benches
	2
	

	Bench Grinder
	1
	1
	

	Battery Bank (12V/24V) for Starting System Practice
	2
	1
	

	Total
	20
	


D. Major Tools & Measuring Instruments (15 Marks)
	Tool / Instrument
	Minimum Quantity
	Marks
	Obtained

	Complete Generator Mechanic Tool Kits (Spanners, Socket Sets, Screwdrivers, Pliers, Allen Keys, Hammers etc.)
	25 sets
	2
	

	Torque Wrenches
	5
	1
	

	Digital Multimeters
	10
	1
	

	Clamp Meters
	5
	1
	

	Insulation Resistance Tester (Megger)
	2
	1
	

	Battery Hydrometer & Battery Load Tester
	2
	1
	

	Compression Test Kit (Diesel Engines)
	2
	1
	

	Injector Nozzle Tester / Injector Servicing Kit
	1
	1
	

	Bearing Puller Sets
	5
	1
	

	Feeler Gauges
	10
	1
	

	Vernier Calipers & Outside Micrometers
	10
	1
	

	Dial Indicator with Magnetic Base
	2
	1
	

	Crimping Tools & Wire Strippers
	10
	1
	

	Frequency Meter / Tachometer
	2
	1
	

	Personal Protective Equipment (Safety Shoes, Gloves, Goggles, Ear Protection, Coveralls)
	25 Sets
	1
	

	Total
	15
	


E. Relevant Institutional Experience (10 Marks)
	Criteria
	Marks
	Obtained

	Successfully conducted Generator Mechanic, Diesel Engine, Industrial Mechanical or Heavy Equipment Maintenance training programmes during the last five years
	4
	

	Experience in Government-funded Technical Skills Development Projects
	2
	

	Evidence of successful trainee certification and employment/self-employment outcomes
	2
	

	Positive client references and/or third-party evaluation reports
	2
	

	Total
	10
	


GRAND SUMMARY
	Category
	Marks
	Marks Obtained

	Tutor Qualification & Experience
	20
	

	Building Infrastructure
	10
	

	Major Equipment
	20
	

	Major Tools & Measuring Instruments
	15
	

	Relevant Institutional Experience
	10
	

	Total
	75
	


Remarks: 

Recommendation:
The Trade of Generator Mechanic (Levels 1 & 2) for ________________________________________________ is recommended / not recommended / conditionally recommended (mention the conditions in remarks).Signatures:
Team Lead: __________________________________________
Other Member(s):


